# Keychron V4 Max

![Keychron V4 Max](https://cdn.shopify.com/s/files/1/0059/0630/1017/files/Keychron_V4_Max_wireless_QMK_mechanical_keyboard.jpg?v=1715227166)

A customizable keyboard.

* Keyboard Maintainer: [Keychron](https://github.com/keychron)
* Hardware Supported: Keychron V4 Max
* Hardware Availability: [Keychron V4 Max QMK/VIA Wireless Custom Mechanical Keyboard](https://www.keychron.com/products/keychron-v4-max-qmk-via-wireless-custom-mechanical-keyboard)

Make example for this keyboard (after setting up your build environment):

    make keychron/v4_max/ansi:default
    make keychron/v4_max/iso:default

Flashing example for this keyboard:

    make keychron/v4_max/ansi_encoder:default:flash
    make keychron/v4_max/iso_encoder:default:flash

**Reset Key**: Toggle mode switch to "Cable", hold down the *Esc* key or reset button underneath space bar while connecting the USB cable,

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
